# (c) Copyright 2023 by Coinkite Inc. This file is covered by license found in COPYING-CC.
#
# Q1 .. mostly same as Mk4
#

BOARD = COLDCARD_Q1
FIRMWARE_BASE   = 0x08020000
BOOTLOADER_BASE = 0x08000000
HW_MODEL = q1
PARENT_MKFILE = Q1-Makefile

# This is release of the bootloader that will be built into the factory.dfu
BOOTLOADER_VERSION = 1.1.0
BOOTLOADER_DIR = q1-bootloader

LATEST_RELEASE = $(shell ls -t1 ../releases/*-q1-*.dfu | head -1)

# Our version for this release.
VERSION_STRING = 6.5.0QX

# Remove this closer to shipping.
#$(warning "Forcing debug build")
#DEBUG_BUILD ?= 1

# keep near top, because defined default target (all)
include shared.mk

# In another window: 
#
#		openocd -f openocd-q1.cfg
#
# Can do:
# - "load" which writes the flash (medium speed, lots of output on st-util)
# - "cont" starts/continues system
# - "br main" sets breakpoints
# - "mon reset" to reset micro
# - and so on
#
debug:
	arm-none-eabi-gdb $(BUILD_DIR)/firmware.elf -x gogo-q1.gdb

# EOF
