--- instance0 ---
recv 0x345 00ff
recv 0x3700 ee
recv 0x345 01ff01ff
recv 0x3701 eeee
recv 0x345 02ff02ff02ff
recv 0x3702 eeeeee
receiver configured single ext id
recv 0x12345678 0102030405
recv 0x12345678 010203
receiver configured single std id
recv 0x505 060708090a0b
recv 0x505 040506
receiver configured ext+std ids
recv 0x12345678 0102030405
recv 0x505 060708090a0b
recv 0x12345678 010203
recv 0x505 040506
receiver configured std+ext ids
recv 0x12345678 0102030405
recv 0x505 060708090a0b
recv 0x12345678 010203
recv 0x505 040506
receiver configured accept none
receiver configured accept all
recv 0x12345678 0102030405
recv 0x2345678 0000
recv 0x678 0001
recv 0x505 060708090a0b
recv 0x345 0002
recv 0x12345679 0003
recv 0x3705 0004
recv 0x12345678 010203
recv 0x505 040506
recv 0x505 0005
recv 0x507 0006
recv 0x13345678 0007
recv 0x12345670 0008
receiver configured accept none again
--- instance1 ---
Sending ID ranges...
Sending for single ext id...
Sending for single std id...
Sending for ext+std ids...
Sending for std+ext ids...
Sending for accept none...
Sending for accept all...
Sending for accept none again...
Sender done
